{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":2,"rows_kept":19,"merged":[[0,0,0,2],[1,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[6,1,6,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2]],"flags":["formulas_cached_only"]}
["    PINGDINGSHAN AOSIDA TECHNOLOGY CO.,LTD"]
["MID, 2ND SHAHE ROAD, YE COUNTY,YE COUNTY,  PINGDINGSHAN CHEMICAL INDUSTRY GATHERING AREA"]
[",HENAN PROVINCE,CHINA. Tel:375 6150809  Fax:375 6110608  Email:asd_jack@pdsasd.com"]
[]
["         Technical Data Sheet             "]
[]
["Product Name: NNO-CL"]
[]
["Item","Data"]
["   Form","Powder"]
["   Colour","Tan"]
["Moisture content / %                                 ≤","9"]
["Dispersion force  / %                                ≥","100"]
["Sodium sulphate content  / %                    ≤","18"]
["Water insoluble matter  / %                       ≤","0.1"]
["Calcium and magnesium ions  / %             ≤","0.15"]
["Fineness(300μm)  / %                              ≤","5"]
["   Ph value (1:100) ","  7-9"]
["Formaldehyde content / (mg/kg)               ≥","200"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}